HTTP测试用例

AT+CIPSEND

1. 百度

GET / HTTP/1.1

Host: [www.baidu.com](http://www.baidu.com)

Connection: close

1. Espressif

POST /v1/datastreams/cpu/datapoint/ HTTP/1.1

Host: iot.espressif.cn

Authorization: token b79ac52f7e6a159768d8ccec90c5b5d8728d41ef

Content-Type: application/x-www-form-urlencoded

Content-Length: 21

Connection: Keep-Alive

{"datapoint":{"x":1}}

1. Activate

POST /v1/device/activate/ HTTP/1.1

Host: iot.espressif.cn

Authorization: token b79ac52f7e6a159768d8ccec90c5b5d8728d41ef

Connection: Keep-Alive

{"encrypt\_method": "PLAIN", "token": " b79ac52f7e6a159768d8ccec90c5b5d8728d41ef "}

1. Yeelink GET

GET /v1.0/device/19465/sensor/34147/datapoints HTTP/1.1

Host: api.yeelink.net

U-ApiKey: ee73a5df716ec70702b14b96ec26fb17

Connection: Keep-Alive

1. Yeelink POST

POST /v1.0/device/19465/sensor/34148/datapoints HTTP/1.1

Host: api.yeelink.net

U-ApiKey: ee73a5df716ec70702b14b96ec26fb17

Content-Type: application/x-www-form-urlencoded

Content-Length: 14

Connection: Keep-Alive

{"value":22.3}

1. Yeelink POST2

POST /v1.0/device/19465/sensor/34148/datapoints HTTP/1.1

Host: api.yeelink.net

Accept: \*/\*

U-ApiKey: ee73a5df716ec70702b14b96ec26fb17

Content-Length: 14

Content-Type: application/x-www-form-urlencoded

{"value":22.3}

1. 常用指令

AT+RST

AT+CWJAP="606","12345678"

AT+CIFSR

AT+CIPSTART="TCP","api.yeelink.net",80

AT+CIPMODE=1

AT+CIPSEND